|  |
| --- |
| Treatments |
| *Control (Bamfield water)* |
| *6 µg/L Copper* |
| *20 µg/L Lead*  |
| *25 µg/L Zinc* |
| *6 µg/L Cu + 8 mg DOC/L PORT*  |
| *6 µg/L Cu + 8 mg DOC/L BAM*  |
| *6 µg/L Cu + 8 mg DOC/L PAC*  |
| *6 µg/L Cu + 8 mg DOC/L Off-CA* |
| *6 µg/L Cu + 8 mg DOC/L Off-BR*  |
| *20 µg/L Pb + 8 mg DOC/L PORT*  |
| *20 µg/L Pb + 8 mg DOC/L BAM*  |
| *20 µg/L Pb + 8 mg DOC/L PAC*  |
| *20 µg/L Pb + 8 mg DOC/L Off-CA*  |
| *20 µg/L Pb + 8 mg DOC/L Off-BR*  |
| *25 µg/L Zn + 8 mg DOC/L PORT*  |
| *25 µg/L Zn + 8 mg DOC/L BAM*  |
| *25 µg/L Zn + 8 mg DOC/L PAC*  |
| *25 µg/L Zn + 8 mg DOC/L Off-CA* |
| *25 µg/L Zn + 8 mg DOC/L Off-BR*  |