Comparison of reaction times from Presentation software against a Matlab code that detected the sound envelope of the voice signal

|  |  |
| --- | --- |
| RT obtained from Matlab code | RT obtained from Presentation Software |
| RT = 0.326 s | RT = 0.329 s |
| RT = 0.296 s | RT = 0.298 s |
| RT = 0.326 s | RT = 0. 329 s |