Supplement 1

Tubes I, II, and III loading-displacement curves and respective the polynomial regressions obtained from two samples of each tube by the Instron Universal Testing Instrument, model 1125 with its original outputs in *kgf*. Conversions to *N* used in the study were based on the factor 1 *kgf* = 9.80665 *N*.





