.. include:: replace.txt


++++++++++++++++++
User Documentation
++++++++++++++++++


Background
----------



We assume the reader is already familiar with how to use the ns-3
simulator to run generic simulation programs. If this is not the case,
we strongly recommend the reader to consult [ns3tutorial]_.

  
Usage Overview
--------------

The ns-3 LTE model is a software library that allows the simulation of
LTE networks, optionally including the Evolved Packet Core (EPC).  The
process of performing such simulations typically involves the
following steps:

 1. *Define the scenario* to be simulated
 2. *Write a simulation program* that recreates the desired scenario
    topology/architecture. This is done accessing the ns-3 LTE model
    library using the ``ns3::LteHelper`` API defined in ``src/lte/helper/lte-helper.h``. 
 3. *Specify configuration parameters* of the objects that are being
    used for the simulation. This can be done using input files (via the
    ``ns3::ConfigStore``) or directly within the simulation program.
 4. *Configure the desired output* to be produced by the simulator
 5. *Run* the simulation.

All these aspects will be explained in the following sections by means
of practical examples.



.. _sec-basic-simulation-program:

Basic simulation program
------------------------

Here is the minimal simulation program that is needed to do an LTE-only simulation (without EPC).

.. highlight:: none

#. Initial boilerplate::
       
    #include <ns3/core-module.h>
    #include <ns3/network-module.h>
    #include <ns3/mobility-module.h>
    #include <ns3/lte-module.h>   

    using namespace ns3;    

    int main (int argc, char *argv[])
    {
      // the rest of the simulation program follows


#. Create an ``LteHelper`` object::

      Ptr<LteHelper> lteHelper = CreateObject<LteHelper> ();

   This will instantiate some common
   objects (e.g., the Channel object) and provide the methods to add
   eNBs and UEs and configure them.

#. Create ``Node`` objects for the eNB(s) and the UEs::

      NodeContainer enbNodes;
      enbNodes.Create (1);
      NodeContainer ueNodes;
      ueNodes.Create (2);
  
   Note that the above Node instances at this point still don't have
   an LTE protocol stack installed; they're just empty nodes. 

#. Configure the Mobility model for all the nodes::

      MobilityHelper mobility;
      mobility.SetMobilityModel ("ns3::ConstantPositionMobilityModel");
      mobility.Install (enbNodes);
      mobility.SetMobilityModel ("ns3::ConstantPositionMobilityModel");
      mobility.Install (ueNodes);

   The above will place all nodes at the coordinates (0,0,0). Please
   refer to the documentation of the ns-3 mobility model for how to
   set your own position or configure node movement.
  
#. Install an LTE protocol stack on the eNB(s)::

      NetDeviceContainer enbDevs;
      enbDevs = lteHelper->InstallEnbDevice (enbNodes);

#. Install an LTE protocol stack on the UEs::

      NetDeviceContainer ueDevs;
      ueDevs = lteHelper->InstallUeDevice (ueNodes);


#. Attach the UEs to an eNB. This will configure each UE according to
   the eNB configuration, and create an RRC connection between them::

      lteHelper->Attach (ueDevs, enbDevs.Get (0));

#. Activate a data radio bearer between each UE and the eNB it is attached to::

      enum EpsBearer::Qci q = EpsBearer::GBR_CONV_VOICE;
      EpsBearer bearer (q);
      lteHelper->ActivateDataRadioBearer (ueDevs, bearer);

   this method will also activate two saturation traffic generators for
   that bearer, one in uplink and one in downlink. 

#. Set the stop time::

       Simulator::Stop (Seconds (0.005));
  
   This is needed otherwise the simulation will last forever, because
   (among others) the start-of-subframe event is scheduled repeatedly, and the
   ns-3 simulator scheduler will hence never run out of events.

#. Run the simulation::

       Simulator::Run ();

#. Cleanup and exit::


       Simulator::Destroy ();
       return 0;
       }

For how to compile and run simulation programs, please refer to [ns3tutorial]_.


Configuration of LTE model parameters
-------------------------------------

All the relevant LTE model parameters are managed through the ns-3
attribute system. Please refer to the [ns3tutorial]_ and [ns3manual]_
for detailed information on all the possible methods to do it
(environmental variables, C++ API, GtkConfigStore...).

In the following, we just briefly summarize
how to do it using input files together with the ns-3 ConfigStore.
First of all, you need to put the following in your simulation
program, right after ``main ()`` starts::

      CommandLine cmd;
      cmd.Parse (argc, argv);
      ConfigStore inputConfig;
      inputConfig.ConfigureDefaults ();
      // parse again so you can override default values from the command line
      cmd.Parse (argc, argv);

for the above to work, make sure you also ``#include "ns3/config-store.h"``.
Now create a text file named (for example) ``input-defaults.txt``
specifying the new default values that you want to use for some attributes::

   default ns3::LteHelper::Scheduler "ns3::PfFfMacScheduler"
   default ns3::LteHelper::PathlossModel "ns3::FriisSpectrumPropagationLossModel"
   default ns3::LteEnbNetDevice::UlBandwidth "25"
   default ns3::LteEnbNetDevice::DlBandwidth "25"
   default ns3::LteEnbNetDevice::DlEarfcn "100"
   default ns3::LteEnbNetDevice::UlEarfcn "18100"
   default ns3::LteUePhy::TxPower "10"
   default ns3::LteUePhy::NoiseFigure "9"
   default ns3::LteEnbPhy::TxPower "30"
   default ns3::LteEnbPhy::NoiseFigure "5"

Supposing your simulation program is called
``src/lte/examples/lte-sim-with-input``, you can now pass these
settings to the simulation program in the following way::

   ./waf --command-template="%s --ns3::ConfigStore::Filename=input-defaults.txt --ns3::ConfigStore::Mode=Load --ns3::ConfigStore::FileFormat=RawText" --run src/lte/examples/lte-sim-with-input


Furthermore, you can generate a template input file with the following
command::

   ./waf --command-template="%s --ns3::ConfigStore::Filename=input-defaults.txt --ns3::ConfigStore::Mode=Save --ns3::ConfigStore::FileFormat=RawText" --run src/lte/examples/lte-sim-with-input

note that the above will put in the file ``input-defaults.txt`` *all*
the default values that are registered in your particular build of the
simulator, including lots of non-LTE attributes.

Configure LTE MAC Scheduler
---------------------------

There are several types of LTE MAC scheduler user can choose here. User can use following codes to define scheduler type::

 Ptr<LteHelper> lteHelper = CreateObject<LteHelper> ();
 lteHelper->SetSchedulerType ("ns3::FdMtFfMacScheduler");    // FD-MT scheduler
 lteHelper->SetSchedulerType ("ns3::TdMtFfMacScheduler");    // TD-MT scheduler
 lteHelper->SetSchedulerType ("ns3::TtaFfMacScheduler");     // TTA scheduler
 lteHelper->SetSchedulerType ("ns3::FdBetFfMacScheduler");   // FD-BET scheduler 
 lteHelper->SetSchedulerType ("ns3::TdBetFfMacScheduler");   // TD-BET scheduler 
 lteHelper->SetSchedulerType ("ns3::FdTbfqFfMacScheduler");  // FD-TBFQ scheduler
 lteHelper->SetSchedulerType ("ns3::TdTbfqFfMacScheduler");  // TD-TBFQ scheduler
 lteHelper->SetSchedulerType ("ns3::PssFfMacScheduler");     //PSS scheduler

TBFQ and PSS have more parameters than other schedulers. Users can define those parameters in following way::

 * TBFQ scheduler::

  Ptr<LteHelper> lteHelper = CreateObject<LteHelper> ();
  lteHelper->SetSchedulerAttribute("DebtLimit", IntegerValue(yourvalue)); // default value -625000 bytes (-5Mb)
  lteHelper->SetSchedulerAttribute("CreditLimit", UintegerValue(yourvalue)); // default value 625000 bytes (5Mb)
  lteHelper->SetSchedulerAttribute("TokenPoolSize", UintegerValue(yourvalue)); // default value 1 byte
  lteHelper->SetSchedulerAttribute("CreditableThreshold", UintegerValue(yourvalue)); // default value 0

 * PSS scheduler::

  Ptr<LteHelper> lteHelper = CreateObject<LteHelper> ();
  lteHelper->SetSchedulerAttribute("nMux", UIntegerValue(yourvalue)); // the maximum number of UE selected by TD scheduler
  lteHelper->SetSchedulerAttribute("PssFdSchedulerType", StringValue("CoItA")); // PF scheduler type in PSS

In TBFQ, default values of debt limit and credit limit are set to -5Mb and 5Mb respectively based on paper [FABokhari2009]_. 
Current implementation does not consider credit threshold (:math:`C` = 0). In PSS, if user does not define nMux, 
PSS will set this value to half of total UE. The default FD scheduler is PFsch.

In addition, token generation rate in TBFQ and target bit rate in PSS need to be configured by Guarantee Bit Rate (GBR) or 
Maximum Bit Rate (MBR) in epc bearer QoS parameters. Users can use following codes to define GBR and MBR in both downlink and uplink::

  Ptr<LteHelper> lteHelper = CreateObject<LteHelper> ();
  enum EpsBearer::Qci q = EpsBearer::yourvalue;  // define Qci type
  GbrQosInformation qos;
  qos.gbrDl = yourvalue; // Downlink GBR
  qos.gbrUl = yourvalue; // Uplink GBR
  qos.mbrDl = yourvalue; // Downlink MBR
  qos.mbrUl = yourvalue; // Uplink MBR
  EpsBearer bearer (q, qos);
  lteHelper->ActivateEpsBearer (ueDevs, bearer, EpcTft::Default ());

In PSS, TBR is obtained from GBR in bearer level QoS parameters. In TBFQ, token generation rate is obtained from the MBR
setting in bearer level QoS parameters, which therefore needs to be configured consistently.
For constant bit rate (CBR) traffic, it is suggested to set MBR to GBR. For variance bit rate (VBR) traffic, 
it is suggested to set MBR k times larger than GBR in order to cover the peak traffic rate. In current implementation, k is set to 
three based on paper [FABokhari2009]_. In addition, current version of TBFQ does not consider RLC header and PDCP header length in 
MBR and GBR. Another parameter in TBFQ is packet arrival rate. This parameter is calculated within scheduler and equals to the past
average throughput which is used in PF scheduler.

Many useful attributes of the LTE-EPC model will be described in the
following subsections. Still, there are many attributes which are not
explicitly mentioned in the design or user documentation, but which
are clearly documented using the ns-3 attribute system. You can easily
print a list of the attributes of a given object together with their
description and default value passing ``--PrintAttributes=`` to a simulation
program, like this::

     ./waf --run lena-simple --command-template="%s --PrintAttributes=ns3::LteHelper"


You can try also with other LTE and EPC objects, like this::
   
     ./waf --run lena-simple --command-template="%s --PrintAttributes=ns3::LteEnbNetDevice"
     ./waf --run lena-simple --command-template="%s --PrintAttributes=ns3::LteEnbMac"
     ./waf --run lena-simple --command-template="%s --PrintAttributes=ns3::LteEnbPhy"
     ./waf --run lena-simple --command-template="%s --PrintAttributes=ns3::LteUePhy"
     ./waf --run lena-simple --command-template="%s --PrintAttributes=ns3::PointToPointEpcHelper"
 


.. _sec-simulation-output:

Simulation Output
-----------------

The ns-3 LTE model currently supports the output to file of PHY, MAC, RLC
and PDCP level Key Performance Indicators (KPIs). You can enable it in
the following way::

      Ptr<LteHelper> lteHelper = CreateObject<LteHelper> ();
      
      // configure all the simulation scenario here...
      
      lteHelper->EnablePhyTraces ();
      lteHelper->EnableMacTraces ();
      lteHelper->EnableRlcTraces ();   
      lteHelper->EnablePdcpTraces ();   

      Simulator::Run ();


RLC and PDCP KPIs are calculated over a time interval and stored on ASCII
files, two for RLC KPIs and two for PDCP KPIs, in each case one for
uplink and one for downlink. The time interval duration can be controlled using the attribute
``ns3::RadioBearerStatsCalculator::EpochDuration``.

The columns of the RLC KPI files is the following (the same
for uplink and downlink):
 
  1. start time of measurement interval in seconds since the start of simulation
  2. end time of measurement interval in seconds since the start of simulation
  3. Cell ID
  4. unique UE ID (IMSI)
  5. cell-specific UE ID (RNTI)
  6. Logical Channel ID
  7. Number of transmitted RLC PDUs
  8. Total bytes transmitted.
  9. Number of received RLC PDUs
  10. Total bytes received
  11. Average RLC PDU delay in seconds
  12. Standard deviation of the RLC PDU delay
  13. Minimum value of the RLC PDU delay
  14. Maximum value of the RLC PDU delay
  15. Average RLC PDU size, in bytes
  16. Standard deviation of the RLC PDU size
  17. Minimum RLC PDU size
  18. Maximum RLC PDU size

Similarly, the columns of the PDCP KPI files is the following (again, the same
for uplink and downlink):
 
  1. start time of measurement interval in seconds since the start of simulation
  2. end time of measurement interval in seconds since the start of simulation
  3. Cell ID
  4. unique UE ID (IMSI)
  5. cell-specific UE ID (RNTI)
  6. Logical Channel ID
  7. Number of transmitted PDCP PDUs
  8. Total bytes transmitted.
  9. Number of received PDCP PDUs
  10. Total bytes received
  11. Average PDCP PDU delay in seconds
  12. Standard deviation of the PDCP PDU delay
  13. Minimum value of the PDCP PDU delay
  14. Maximum value of the PDCP PDU delay
  15. Average PDCP PDU size, in bytes
  16. Standard deviation of the PDCP PDU size
  17. Minimum PDCP PDU size
  18. Maximum PDCP PDU size



MAC KPIs are basically a trace of the resource allocation reported by
the scheduler upon the start of every subframe. They are stored in
ASCII files. For downlink MAC KPIs the format is the following:

  1. Simulation time in seconds at which the allocation is indicated by the scheduler
  2. Cell ID
  3. unique UE ID (IMSI)
  4. Frame number
  5. Subframe number
  6. cell-specific UE ID (RNTI)
  7. MCS of TB 1
  8. size of TB 1
  9. MCS of TB 2 (0 if not present)
  10. size of TB 2 (0 if not present)

while for uplink MAC KPIs the format is:

  1. Simulation time in seconds at which the allocation is indicated by the scheduler
  2. Cell ID
  3. unique UE ID (IMSI)
  4. Frame number
  5. Subframe number
  6. cell-specific UE ID (RNTI)
  7. MCS of TB
  8. size of TB

The names of the files used for MAC KPI output can be customized via
the ns-3 attributes ``ns3::MacStatsCalculator::DlOutputFilename`` and 
``ns3::MacStatsCalculator::UlOutputFilename``.

PHY KPIs are distributed in seven different files, configurable through the attributes

  1. ``ns3::PhyStatsCalculator::DlRsrpSinrFilename``
  2. ``ns3::PhyStatsCalculator::UeSinrFilename``
  3. ``ns3::PhyStatsCalculator::InterferenceFilename``
  4. ``ns3::PhyStatsCalculator::DlTxOutputFilename``
  5. ``ns3::PhyStatsCalculator::UlTxOutputFilename``
  6. ``ns3::PhyStatsCalculator::DlRxOutputFilename``
  7. ``ns3::PhyStatsCalculator::UlRxOutputFilename``


In the RSRP/SINR file, the following content is available:

  1. Simulation time in seconds at which the allocation is indicated by the scheduler
  2. Cell ID
  3. unique UE ID (IMSI)
  4. RSRP
  5. Linear average over all RBs of the downlink SINR in linear units

The contents in the UE SINR file are:

  1. Simulation time in seconds at which the allocation is indicated by the scheduler
  2. Cell ID
  3. unique UE ID (IMSI)
  4. uplink SINR in linear units for the UE

In the interference filename the content is:

  1. Simulation time in seconds at which the allocation is indicated by the scheduler
  2. Cell ID
  3. List of interference values per RB

In UL and DL transmission files the parameters included are:

  1. Simulation time in milliseconds
  2. Cell ID
  3. unique UE ID (IMSI)
  4. RNTI
  5. Layer of transmission
  6. MCS
  7. size of the TB
  8. Redundancy version
  9. New Data Indicator flag

And finally, in UL and DL reception files the parameters included are:

  1. Simulation time in milliseconds
  2. Cell ID
  3. unique UE ID (IMSI)
  4. RNTI
  5. Transmission Mode
  6. Layer of transmission
  7. MCS
  8. size of the TB
  9. Redundancy version
  10. New Data Indicator flag
  11. Correctness in the reception of the TB


Fading Trace Usage
------------------

In this section we will describe how to use fading traces within LTE simulations.

Fading Traces Generation
************************


It is possible to generate fading traces by using a dedicated matlab script provided with the code (``/lte/model/fading-traces/fading-trace-generator.m``). This script already includes the typical taps configurations for three 3GPP scenarios (i.e., pedestrian, vehicular and urban as defined in Annex B.2 of [TS36104]_); however users can also introduce their specific configurations. The list of the configurable parameters is provided in the following:

 * ``fc`` : the frequency in use (it affects the computation of the doppler speed).
 * ``v_km_h`` : the speed of the users
 * ``traceDuration`` : the duration in seconds of the total length of the trace.
 * ``numRBs`` : the number of the resource block to be evaluated. 
 * ``tag`` : the tag to be applied to the file generated.

The file generated contains ASCII-formatted real values organized in a matrix fashion: every row corresponds to a different RB, and every column correspond to a different temporal fading trace sample.

It has to be noted that the ns-3 LTE module is able to work with any fading trace file that complies with the above described ASCII format. Hence, other external tools can be used to generate custom fading traces, such as for example other simulators or experimental devices.

Fading Traces Usage
*******************

When using a fading trace, it is of paramount importance to specify correctly the trace parameters in the simulation, so that the fading model can load and use it correcly.
The parameters to be configured are:

 * ``TraceFilename`` : the name of the trace to be loaded (absolute path, or relative path w.r.t. the path from where the simulation program is executed);
 * ``TraceLength`` : the trace duration in seconds;
 * ``SamplesNum`` : the number of samples;
 * ``WindowSize`` : the size of the fading sampling window in seconds;

It is important to highlight that the sampling interval of the fading trace has to be 1 ms or greater, and in the latter case it has to be an integer multiple of 1 ms in order to be correctly processed by the fading module.

The default configuration of the matlab script provides a trace 10 seconds long, made of 10,000 samples (i.e., 1 sample per TTI=1ms) and used with a windows size of 0.5 seconds amplitude. These are also the default values of the parameters above used in the simulator; therefore their settage can be avoided in case the fading trace respects them.

In order to activate the fading module (which is not active by default) the following code should be included in the simulation program::

  Ptr<LteHelper> lteHelper = CreateObject<LteHelper> ();
  lteHelper->SetFadingModel("ns3::TraceFadingLossModel");

And for setting the parameters::

  lteHelper->SetFadingModelAttribute ("TraceFilename", StringValue ("src/lte/model/fading-traces/fading_trace_EPA_3kmph.fad"));
  lteHelper->SetFadingModelAttribute ("TraceLength", TimeValue (Seconds (10.0)));
  lteHelper->SetFadingModelAttribute ("SamplesNum", UintegerValue (10000));
  lteHelper->SetFadingModelAttribute ("WindowSize", TimeValue (Seconds (0.5)));
  lteHelper->SetFadingModelAttribute ("RbNum", UintegerValue (100));

It has to be noted that, ``TraceFilename`` does not have a default value, therefore is has to be always set explicitly.

The simulator provide natively three fading traces generated according to the configurations defined in in Annex B.2 of [TS36104]_. These traces are available in the folder ``src/lte/model/fading-traces/``). An excerpt from these traces is represented in the following figures.


.. _fig-fadingPedestrianTrace:

.. figure:: figures/fading_pedestrian.*                 
   :align: center
   :alt: Fading trace 3 kmph

   Excerpt of the fading trace included in the simulator for a pedestrian scenario (speed of 3 kmph).

.. _fig-fadingVehicularTrace:

.. figure:: figures/fading_vehicular.*                 
   :align: center
   :alt: Fading trace 60 kmph

   Excerpt of the fading trace included in the simulator for a vehicular  scenario (speed of 60 kmph).

.. _fig-fadingUrbanTrace:

.. figure:: figures/fading_urban_3kmph.*                 
   :align: center
   :alt: Fading trace 3 kmph

   Excerpt of the fading trace included in the simulator for an urban  scenario (speed of 3 kmph).


Mobility Model with Buildings
-----------------------------

We now explain by examples how to use the buildings model (in particular, the ``MobilityBuildingInfo`` and the ``BuildingPropagationModel`` classes) in an ns-3 simulation program to setup an LTE simulation scenario that includes buildings and indoor nodes.


.. highlight:: none

#. Header files to be included::

    #include <ns3/mobility-building-info.h>
    #include <ns3/buildings-propagation-loss-model.h>
    #include <ns3/building.h>

#. Pathloss model selection::

    Ptr<LteHelper> lteHelper = CreateObject<LteHelper> ();
  
    lteHelper->SetAttribute ("PathlossModel", StringValue ("ns3::BuildingsPropagationLossModel"));

#. EUTRA Band Selection
   
The selection of the working frequency of the propagation model has to be done with the standard ns-3 attribute system as described in the correspond section ("Configuration of LTE model parameters") by means of the DlEarfcn and UlEarfcn parameters, for instance::

   lteHelper->SetEnbDeviceAttribute ("DlEarfcn", UintegerValue (100));
   lteHelper->SetEnbDeviceAttribute ("UlEarfcn", UintegerValue (18100));

It is to be noted that using other means to configure the frequency used by the propagation model (i.e., configuring the corresponding BuildingsPropagationLossModel attributes directly) might generates conflicts in the frequencies definition in the modules during the simulation, and is therefore not advised.

#. Mobility model selection::

    MobilityHelper mobility;
    mobility.SetMobilityModel ("ns3::ConstantPositionMobilityModel"); 

    It is to be noted that any mobility model can be used. 

#. Building creation::

    double x_min = 0.0;
    double x_max = 10.0;
    double y_min = 0.0;
    double y_max = 20.0;
    double z_min = 0.0;
    double z_max = 10.0;
    Ptr<Building> b = CreateObject <Building> ();
    b->SetBoundaries (Box (x_min, x_max, y_min, y_max, z_min, z_max));
    b->SetBuildingType (Building::Residential);
    b->SetExtWallsType (Building::ConcreteWithWindows);
    b->SetNFloors (3);
    b->SetNRoomsX (3);
    b->SetNRoomsY (2);

   This will instantiate a residential building with base of 10 x 20 meters and height of 10 meters whose external walls are of concrete with windows; the building has three floors and has an internal 3 x 2  grid of rooms of equal size.

#. Node creation and positioning::

    ueNodes.Create (2);
    mobility.Install (ueNodes);
    BuildingsHelper::Install (ueNodes);
    NetDeviceContainer ueDevs;
    ueDevs = lteHelper->InstallUeDevice (ueNodes);
    Ptr<ConstantPositionMobilityModel> mm0 = enbNodes.Get (0)->GetObject<ConstantPositionMobilityModel> ();
    Ptr<ConstantPositionMobilityModel> mm1 = enbNodes.Get (1)->GetObject<ConstantPositionMobilityModel> ();
    mm0->SetPosition (Vector (5.0, 5.0, 1.5));
    mm1->SetPosition (Vector (30.0, 40.0, 1.5));

#. Finalize the building and mobility model configuration::

    BuildingsHelper::MakeMobilityModelConsistent ();

See the documentation of the *buildings* module for more detailed information.


PHY Error Model
---------------

The Physical error model consists of the data error model and the downlink control error model, both of them active by default. It is possible to deactivate them with the ns3 attribute system, in detail::

  Config::SetDefault ("ns3::LteSpectrumPhy::CtrlErrorModelEnabled", BooleanValue (false));
  Config::SetDefault ("ns3::LteSpectrumPhy::DataErrorModelEnabled", BooleanValue (false));  




MIMO Model
----------

Is this subsection we illustrate how to configure the MIMO parameters. LTE defines 7 types of transmission modes:

 * Transmission Mode 1: SISO.
 * Transmission Mode 2: MIMO Tx Diversity.
 * Transmission Mode 3: MIMO Spatial Multiplexity Open Loop.
 * Transmission Mode 4: MIMO Spatial Multiplexity Closed Loop.
 * Transmission Mode 5: MIMO Multi-User.
 * Transmission Mode 6: Closer loop single layer precoding.
 * Transmission Mode 7: Single antenna port 5.

According to model implemented, the simulator includes the first three transmission modes types. The default one is the Transmission Mode 1 (SISO). In order to change the default Transmission Mode to be used, the attribute ``DefaultTransmissionMode`` of the ``LteEnbRrc`` can be used, as shown in the following::

  Config::SetDefault ("ns3::LteEnbRrc::DefaultTransmissionMode", UintegerValue (0)); // SISO
  Config::SetDefault ("ns3::LteEnbRrc::DefaultTransmissionMode", UintegerValue (1)); // MIMO Tx diversity (1 layer)
  Config::SetDefault ("ns3::LteEnbRrc::DefaultTransmissionMode", UintegerValue (2)); // MIMO Spatial Multiplexity (2 layers)

For changing the transmission mode of a certain user during the simulation a specific interface has been implemented in both standard schedulers::

  void TransmissionModeConfigurationUpdate (uint16_t rnti, uint8_t txMode);

This method can be used both for developing transmission mode decision engine (i.e., for optimizing the transmission mode according to channel condition and/or user's requirements) and for manual switching from simulation script. In the latter case, the switching can be done as shown in the following::

  Ptr<LteEnbNetDevice> lteEnbDev = enbDevs.Get (0)->GetObject<LteEnbNetDevice> ();
  PointerValue ptrval;
  enbNetDev->GetAttribute ("FfMacScheduler", ptrval);
  Ptr<RrFfMacScheduler> rrsched = ptrval.Get<RrFfMacScheduler> ();
  Simulator::Schedule (Seconds (0.2), &RrFfMacScheduler::TransmissionModeConfigurationUpdate, rrsched, rnti, 1);

Finally, the model implemented can be reconfigured according to different MIMO models by updating the gain values (the only constraints is that the gain has to be constant during simulation run-time and common for the layers). The gain of each Transmission Mode can be changed according to the standard ns3 attribute system, where the attributes are: ``TxMode1Gain``, ``TxMode2Gain``, ``TxMode3Gain``, ``TxMode4Gain``, ``TxMode5Gain``, ``TxMode6Gain`` and ``TxMode7Gain``. By default only ``TxMode1Gain``, ``TxMode2Gain`` and ``TxMode3Gain`` have a meaningful value, that are the ones derived by _[CatreuxMIMO] (i.e., respectively 0.0, 4.2 and -2.8 dB).
  





Use of AntennaModel
-------------------

We now show how associate a particular AntennaModel with an eNB device
in order to model a sector of a macro eNB. For this purpose, it is
convenient to use the ``CosineAntennaModel`` provided by the ns-3
antenna module. The configuration of the eNB is to be done via the
``LteHelper`` instance right before the creation of the
``EnbNetDevice``, as shown in the following::
  
  lteHelper->SetEnbAntennaModelType ("ns3::CosineAntennaModel");
  lteHelper->SetEnbAntennaModelAttribute ("Orientation", DoubleValue (0));
  lteHelper->SetEnbAntennaModelAttribute ("Beamwidth",   DoubleValue (60);
  lteHelper->SetEnbAntennaModelAttribute ("MaxGain",     DoubleValue (0.0));

the above code will generate an antenna model with a 60 degrees
beamwidth pointing along the X axis. The orientation is measured
in degrees from the X axis, e.g., an orientation of 90 would point
along the Y axis, and an orientation of -90 would point in the
negative direction along the Y axis. The beamwidth is the -3 dB
beamwidth, e.g, for a 60 degree beamwidth the antenna gain at an angle
of :math:`\pm 30` degrees from the direction of orientation is -3 dB.

To create a multi-sector site, you need to create different ns-3 nodes
placed at the same position, and to configure separate ``EnbNetDevice``
with different antenna orientations to be installed on each node.


.. _sec-radio-environment-maps:

Radio Environment Maps
----------------------

By using the class ``RadioEnvironmentMapHelper`` it is possible to output
to a file a Radio Environment Map (REM), i.e., a uniform 2D grid of values
that represent the Signal-to-noise ratio in the downlink with respect
to the eNB that has the strongest signal at each point. 

To do this, you just need to add the following code to your simulation
program towards the end, right before the call to Simulator::Run ()::

  Ptr<RadioEnvironmentMapHelper> remHelper = CreateObject<RadioEnvironmentMapHelper> ();
  remHelper->SetAttribute ("ChannelPath", StringValue ("/ChannelList/0"));
  remHelper->SetAttribute ("OutputFile", StringValue ("rem.out"));
  remHelper->SetAttribute ("XMin", DoubleValue (-400.0));
  remHelper->SetAttribute ("XMax", DoubleValue (400.0));
  remHelper->SetAttribute ("XRes", UintegerValue (100));
  remHelper->SetAttribute ("YMin", DoubleValue (-300.0));
  remHelper->SetAttribute ("YMax", DoubleValue (300.0));
  remHelper->SetAttribute ("YRes", UintegerValue (75));
  remHelper->SetAttribute ("Z", DoubleValue (0.0));
  remHelper->Install ();

By configuring the attributes of the ``RadioEnvironmentMapHelper`` object
as shown above, you can tune the parameters of the REM to be
generated. Note that each ``RadioEnvironmentMapHelper`` instance can
generate only one REM; if you want to generate more REMs, you need to
create one separate instance for each REM. 

Note that the REM generation is very demanding, in particular:

 * the run-time memory consumption is approximately 5KB per pixel. For example,
   a REM with a resolution of 500x500 would need about 1.25 GB of memory, and
   a resolution of 1000x1000 would need needs about 5 GB (too much for a
   regular PC at the time of this writing). To overcome this issue,
   the REM is generated at successive steps, with each step evaluating
   at most a number of pixels determined by the value of the 
   the attribute ``RadioEnvironmentMapHelper::MaxPointsPerIteration``. 
 * if you generate a REM at the beginning of a simulation, it will
   slow down the execution of the rest of the simulation. If you want
   to generate a REM for a program and also use the same program to
   get simulation result, it is recommended to add a command-line
   switch that allows to either generate the REM or run the complete
   simulation. For this purpose, note that there is an attribute
   ``RadioEnvironmentMapHelper::StopWhenDone`` (default: true) that
   will force the simulation to stop right after the REM has been generated.

The REM is stored in an ASCII file in the following format:

 * column 1 is the x coordinate
 * column 2 is the y coordinate
 * column 3 is the z coordinate
 * column 4 is the SINR in linear units

A minimal gnuplot script that allows you to plot the REM is given
below::

   set view map;
   set xlabel "X"
   set ylabel "Y"
   set cblabel "SINR (dB)"
   unset key
   plot "rem.out" using ($1):($2):(10*log10($4)) with image

As an example, here is the REM that can be obtained with the example program lena-dual-stripe, which shows a three-sector LTE macrocell in a co-channel deployment with some residential femtocells randomly deployed in two blocks of apartments.

.. _fig-lena-dual-stripe:

.. figure:: figures/lena-dual-stripe.*
   :align: center

   REM obtained from the lena-dual-stripe example


Note that the lena-dual-stripe example program also generate
gnuplot-compatible output files containing information about the
positions of the UE and eNB nodes as well as of the buildings,
respectively in the files ``ues.txt``, ``enbs.txt`` and
``buildings.txt``. These can be easily included when using
gnuplot. For example, assuming that your gnuplot script (e.g., the
minimal gnuplot script described above) is saved in a file named
``my_plot_script``, running the following command would plot the
location of UEs, eNBs and buildings on top of the REM:: 

   gnuplot -p enbs.txt ues.txt buildings.txt my_plot_script



AMC Model and CQI Calculation
-----------------------------

The simulator provides two possible schemes for what concerns the selection of the MCSs and correspondly the generation of the CQIs. The first one is based on the GSoC module [Piro2011]_ and works per RB basis. This model can be activated with the ns3 attribute system, as presented in the following::

  Config::SetDefault ("ns3::LteAmc::AmcModel", EnumValue (LteAmc::PiroEW2010));

While, the solution based on the physical error model can be controlled with::

  Config::SetDefault ("ns3::LteAmc::AmcModel", EnumValue (LteAmc::MiErrorModel));

Finally, the required efficiency of the ``PiroEW2010`` AMC module can be tuned thanks to the ``Ber`` attribute (), for instance::

  Config::SetDefault ("ns3::LteAmc::Ber", DoubleValue (0.00005));



.. _sec-evolved-packet-core:

Evolved Packet Core (EPC)
-------------------------

We now explain how to write a simulation program that allows to
simulate the EPC in addition to the LTE radio access network. The use
of EPC allows to use IPv4 networking with LTE devices. In other words,
you will be able to use the regular ns-3 applications and sockets over
IPv4 over LTE, and also to connect an LTE network to any other IPv4
network you might have in your simulation.

First of all, in addition to ``LteHelper`` that we already introduced
in :ref:`sec-basic-simulation-program`, you need to use an additional
``EpcHelper`` class, which will take care of creating the EPC entities and
network topology. Note that you can't use ``EpcHelper`` directly, as
it is an abstract base class; instead, you need to use one of its
child classes, which provide different EPC topology implementations. In
this example we will consider ``PointToPointEpcHelper``, which
implements an EPC based on point-to-point links. To use it, you need
first to insert this code in your simulation program::

  Ptr<LteHelper> lteHelper = CreateObject<LteHelper> ();
  Ptr<PointToPointEpcHelper> epcHelper = CreateObject<PointToPointEpcHelper> ();

Then, you need to tell the LTE helper that the EPC will be used::

  lteHelper->SetEpcHelper (epcHelper);

the above step is necessary so that the LTE helper will trigger the
appropriate EPC configuration in correspondance with some important
configuration, such as when a new eNB or UE is added to the
simulation, or an EPS bearer is created. The EPC helper will
automatically take care of the necessary setup, such as S1 link
creation and S1 bearer setup. All this will be done without the
intervention of the user.

Calling ``lteHelper->SetEpcHelper (epcHelper)`` enables the use of
EPC, and has the side effect that any new ``LteEnbRrc`` that is
created will have the ``EpsBearerToRlcMapping`` attribute set to
``RLC_UM_ALWAYS`` instead of ``RLC_SM_ALWAYS`` if the latter was
the default; otherwise, the attribute won't be changed (e.g., if
you changed the default to ``RLC_AM_ALWAYS``, it won't be touched).

It is to be noted that the ``EpcHelper`` will also automatically
create the PGW node and configure it so that it can properly handle
traffic from/to the LTE radio access network.  Still,
you need to add some explicit code to connect the PGW to other
IPv4 networks (e.g., the internet). Here is a very simple example about
how to connect a single remote host to the PGW via a point-to-point
link::

  Ptr<Node> pgw = epcHelper->GetPgwNode ();

   // Create a single RemoteHost
  NodeContainer remoteHostContainer;
  remoteHostContainer.Create (1);
  Ptr<Node> remoteHost = remoteHostContainer.Get (0);
  InternetStackHelper internet;
  internet.Install (remoteHostContainer);

  // Create the internet
  PointToPointHelper p2ph;
  p2ph.SetDeviceAttribute ("DataRate", DataRateValue (DataRate ("100Gb/s")));
  p2ph.SetDeviceAttribute ("Mtu", UintegerValue (1500));
  p2ph.SetChannelAttribute ("Delay", TimeValue (Seconds (0.010)));  
  NetDeviceContainer internetDevices = p2ph.Install (pgw, remoteHost);  
  Ipv4AddressHelper ipv4h;
  ipv4h.SetBase ("1.0.0.0", "255.0.0.0");
  Ipv4InterfaceContainer internetIpIfaces = ipv4h.Assign (internetDevices);
  // interface 0 is localhost, 1 is the p2p device
  Ipv4Address remoteHostAddr = internetIpIfaces.GetAddress (1);
  

It's important to specify routes so that the remote host can reach LTE
UEs. One way of doing this is by exploiting the fact that the
``PointToPointEpcHelper`` will by default assign to LTE UEs an IP address in the
7.0.0.0 network. With this in mind, it suffices to do::

  Ipv4StaticRoutingHelper ipv4RoutingHelper;
  Ptr<Ipv4StaticRouting> remoteHostStaticRouting = ipv4RoutingHelper.GetStaticRouting (remoteHost->GetObject<Ipv4> ());
  remoteHostStaticRouting->AddNetworkRouteTo (Ipv4Address ("7.0.0.0"), Ipv4Mask ("255.0.0.0"), 1);

Now, you should go on and create LTE eNBs and UEs as explained in the
previous sections. You can of course configure other LTE aspects such
as pathloss and fading models. Right after you created the UEs, you
should also configure them for IP networking. This is done as
follows. We assume you have a container for UE and eNodeB nodes like this::

      NodeContainer ueNodes;
      NodeContainer enbNodes;
      

to configure an LTE-only simulation, you would then normally do
something like this::

      NetDeviceContainer ueLteDevs = lteHelper->InstallUeDevice (ueNodes);
      lteHelper->Attach (ueLteDevs, enbLteDevs.Get (0));        

in order to configure the UEs for IP networking, you just need to
additionally do like this::

      // we install the IP stack on the UEs 
      InternetStackHelper internet;
      internet.Install (ueNodes);

      // assign IP address to UEs
      for (uint32_t u = 0; u < ueNodes.GetN (); ++u)
        {
          Ptr<Node> ue = ueNodes.Get (u);          
          Ptr<NetDevice> ueLteDevice = ueLteDevs.Get (u);
          Ipv4InterfaceContainer ueIpIface = epcHelper->AssignUeIpv4Address (NetDeviceContainer (ueLteDevice));
          // set the default gateway for the UE
          Ptr<Ipv4StaticRouting> ueStaticRouting = ipv4RoutingHelper.GetStaticRouting (ue->GetObject<Ipv4> ());          
          ueStaticRouting->SetDefaultRoute (epcHelper->GetUeDefaultGatewayAddress (), 1);
        }

The activation of bearers is done in a slightly different way with
respect to what done for an LTE-only simulation. First, the method
ActivateDataRadioBearer is not to be used when the EPC is
used. Second, when EPC is used, the default EPS bearer will be
activated automatically when you call LteHelper::Attach (). Third, if
you want to setup dedicated EPS bearer, you can do so using the method
LteHelper::ActivateDedicatedEpsBearer (). This method takes as a
parameter the Traffic Flow Template (TFT), which is a struct that
identifies the type of traffic that will be mapped to the dedicated
EPS bearer. Here is an example for how to setup a dedicated bearer
for an application at the UE communicating on port 1234::

      Ptr<EpcTft> tft = Create<EpcTft> ();
      EpcTft::PacketFilter pf;
      pf.localPortStart = 1234;
      pf.localPortEnd = 1234;
      tft->Add (pf);  
      lteHelper->ActivateEpsBearer (ueLteDevs, EpsBearer (EpsBearer::NGBR_VIDEO_TCP_DEFAULT), pf);

you can of course use custom EpsBearer and EpcTft configurations,
please refer to the doxygen documentation for how to do it.


Finally, you can install applications on the LTE UE nodes that communicate
with remote applications over the internet. This is done following the
usual ns-3 procedures. Following our simple example with a single
remoteHost, here is how to setup downlink communication, with an
UdpClient application on the remote host, and a PacketSink on the LTE UE
(using the same variable names of the previous code snippets) ::

       uint16_t dlPort = 1234;
       PacketSinkHelper packetSinkHelper ("ns3::UdpSocketFactory", 
                                          InetSocketAddress (Ipv4Address::GetAny (), dlPort));
       ApplicationContainer serverApps = packetSinkHelper.Install (ue);
       serverApps.Start (Seconds (0.01));
       UdpClientHelper client (ueIpIface.GetAddress (0), dlPort);
       ApplicationContainer clientApps = client.Install (remoteHost);
       clientApps.Start (Seconds (0.01));

That's all! You can now start your simulation as usual::

  Simulator::Stop (Seconds (10.0));  
  Simulator::Run ();



.. _sec-network-attachment:

Network Attachment
------------------

As shown in the basic example in section :ref:`sec-basic-simulation-program`,
attaching a UE to an eNodeB is done by calling ``LteHelper::Attach`` function.

There are 2 possible ways of network attachment. The first method is the
*"manual"* one, while the second one has a more *"automatic"* sense on it. Each
of them will be covered in this section.

Manual attachment
*****************

This method uses the ``LteHelper::Attach`` function mentioned above. It has been
the only available network attachment method in earlier versions of LTE module.
It is typically invoked before the simulation begins::

   lteHelper->Attach (ueDevs, enbDev); // attach one or more UEs to a single eNodeB

``LteHelper::InstallEnbDevice`` and ``LteHelper::InstallUeDevice`` functions
must have been called before attaching. In an EPC-enabled simulation, it is also
required to have IPv4 properly pre-installed in the UE.

This method is very simple, but requires you to know exactly which UE belongs to
to which eNodeB before the simulation begins. This can be difficult when the UE
initial position is randomly determined by the simulation script.

One may choose the distance between the UE and the eNodeB as a criterion for
selecting the appropriate cell. It is quite simple (at least from the
simulator's point of view) and sometimes practical. But it is important to note
that sometimes distance does not make a single correct criterion. For instance,
the eNodeB antenna directivity should be considered as well. Besides that, one
should also take into account the channel condition, which might be fluctuating
if there is fading or shadowing in effect. In these kind of cases, network
attachment should not be based on distance alone.

In real life, UE will automatically evaluate certain criteria and select the
best cell to attach to, without manual intervention from the user. Obviously
this is not the case in this ``LteHelper::Attach`` function. The other network
attachment method uses more *"automatic"* approach to network attachment, as
will be described next.

Automatic attachment using Idle mode cell selection procedure
*************************************************************

The strength of the received signal is the standard criterion used for selecting
the best cell to attach to. The use of this criterion is implemented in the
`initial cell selection` process, which can be invoked by calling another
version of the ``LteHelper::Attach`` function, as shown below::

   lteHelper->Attach (ueDevs); // attach one or more UEs to a strongest cell

The difference with the manual method is that the destination eNodeB is not
specified. The procedure will find the best cell for the UEs, based on several
criteria, including the strength of the received signal (RSRP).

After the method is called, the UE will spend some time to measure the
neighbouring cells, and then attempt to attach to the best one. More details can
be found in section :ref:`sec-initial-cell-selection` of the Design
Documentation.

It is important to note that this method only works in EPC-enabled simulations.
LTE-only simulations must resort to manual attachment method.

Closed Subscriber Group
***********************

An interesting use case of the initial cell selection process is to setup a
simulation environment with Closed Subscriber Group (CSG).

For example, a certain eNodeB, typically a smaller version such as femtocell,
might belong to a private owner (e.g. a household or business), allowing access
only to some UEs which have been previously registered by the owner. The eNodeB
and the registered UEs altogether form a CSG.

The access restriction can be simulated by "labeling" the CSG members with the
same CSG ID. This is done through the attributes in both eNodeB and UE, for
example using the following ``LteHelper`` functions::

   // label the following eNodeBs with CSG identity of 1 and CSG indication enabled
   lteHelper->SetEnbDeviceAttribute ("CsgId", UintegerValue (1));
   lteHelper->SetEnbDeviceAttribute ("CsgIndication", BooleanValue (true));

   // label one or more UEs with CSG identity of 1
   lteHelper->SetUeDeviceAttribute ("CsgId", UintegerValue (1));
   
   // install the eNodeBs and UEs
   NetDeviceContainer csgEnbDevs = lteHelper->InstallEnbDevice (csgEnbNodes);
   NetDeviceContainer csgUeDevs = lteHelper->InstallUeDevice (csgUeNodes);

Then enable the initial cell selection procedure on the UEs:: 

   lteHelper->Attach (csgUeDevs);

This is necessary because the CSG restriction only works with automatic method
of network attachment, but not in the manual method.

Note that setting the CSG indication of an eNodeB as false (the default value)
will disable the restriction, i.e., any UEs can connect to this eNodeB.



.. _sec-configure-ue-measurements:

Configure UE measurements
-------------------------

The active UE measurement configuration in a simulation is dictated by the
selected so called "consumers", such as handover algorithm. Users may add their
own configuration into action, and there are several ways to do so:

 #. direct configuration in eNodeB RRC entity;
 
 #. configuring existing handover algorithm; and
 
 #. developing a new handover algorithm.
 
This section will cover the first method only. The second method is covered in
:ref:`sec-automatic-handover`, while the third method is explained in length in
Section :ref:`sec-handover-algorithm` of the Design Documentation.

Direct configuration in eNodeB RRC works as follows. User begins by creating a
new ``LteRrcSap::ReportConfigEutra`` instance and pass it to the
``LteEnbRrc::AddUeMeasReportConfig`` function. The function will return the
``measId`` (measurement identity) which is a unique reference of the
configuration in the eNodeB instance. This function must be called before the
simulation begins. The measurement configuration will be active in all UEs
attached to the eNodeB throughout the duration of the simulation. During the
simulation, user can capture the measurement reports produced by the UEs by
listening to the existing ``LteEnbRrc::RecvMeasurementReport`` trace source.

The structure `ReportConfigEutra` is in accord with 3GPP specification.
Definition of the structure and each member field can be found in Section 6.3.5
of [TS36331]_.

The code sample below configures Event A1 RSRP measurement to every eNodeB
within the container ``devs``::

   LteRrcSap::ReportConfigEutra config;        
   config.eventId = LteRrcSap::ReportConfigEutra::EVENT_A1;
   config.threshold1.choice = LteRrcSap::ThresholdEutra::THRESHOLD_RSRP;
   config.threshold1.range = 41;
   config.triggerQuantity = LteRrcSap::ReportConfigEutra::RSRP;
   config.reportInterval = LteRrcSap::ReportConfigEutra::MS480;
   
   std::vector<uint8_t> measIdList;

   NetDeviceContainer::Iterator it;
   for (it = devs.Begin (); it != devs.End (); it++)
   {
     Ptr<NetDevice> dev = *it;
     Ptr<LteEnbNetDevice> enbDev = dev->GetObject<LteEnbNetDevice> ();
     Ptr<LteEnbRrc> enbRrc = enbDev->GetRrc ();
    
     uint8_t measId = enbRrc->AddUeMeasReportConfig (config);
     measIdList.push_back (measId); // remember the measId created
    
     enbRrc->TraceConnect ("RecvMeasurementReport",
                           "context",
                           MakeCallback (&RecvMeasurementReportCallback));
   }

Note that thresholds are expressed as range. In the example above, the range 41
for RSRP corresponds to -100 dBm. The conversion from and to the range format is
due to Section 9.1.4 and 9.1.7 of [TS36133]_. The ``EutranMeasurementMapping``
class has several static functions that can be used for this purpose.

The corresponding callback function would have a definition similar as below::

   void
   RecvMeasurementReportCallback (std::string context,
                                  uint64_t imsi,
                                  uint16_t cellId,
                                  uint16_t rnti,
                                  LteRrcSap::MeasurementReport measReport);

This method will register the callback function as a consumer of UE
measurements. In the case where there are more than one consumers in the
simulation (e.g. handover algorithm), the measurements intended for other
consumers will also be captured by this callback function. Users may utilize the
the ``measId`` field, contained within the ``LteRrcSap::MeasurementReport``
argument of the callback function, to tell which measurement configuration has
triggered the report.

In general, this mechanism prevents one consumer to unknowingly intervene with
another consumer's reporting configuration.

Note that only the reporting configuration part (i.e.
``LteRrcSap::ReportConfigEutra``) of the UE measurements parameter is open for
consumers to configure, while the other parts are kept hidden. The
intra-frequency limitation is the main motivation behind this API implementation
decision:

 - there is only one, unambiguous and definitive *measurement object*, thus
   there is no need to configure it;
   
 - *measurement identities* are kept hidden because of the fact that there is
   one-to-one mapping between reporting configuration and measurement identity,
   thus a new measurement identity is set up automatically when a new reporting
   configuration is created;

 - *quantity configuration* is configured elsewhere, see
   :ref:`sec-performing-measurements`; and
   
 - *measurement gaps* are not supported, because it is only applicable for
   inter-frequency settings;



.. _sec-x2-based-handover:

X2-based handover
-----------------

As defined by 3GPP, handover is a procedure for changing the serving cell of a
UE in CONNECTED mode. The two eNodeBs involved in the process are typically
called the *source eNodeB* and the *target eNodeB*.

In order to enable the execution of X2-based handover in simulation, there are
two requirements that must be met. Firstly, EPC must be enabled in the
simulation (see :ref:`sec-evolved-packet-core`).

Secondly, an X2 interface must be configured between the two eNodeBs, which
needs to be done explicitly within the simulation program::

   lteHelper->AddX2Interface (enbNodes);

where ``enbNodes`` is a ``NodeContainer`` that contains the two eNodeBs between
which the X2 interface is to be configured. If the container has more than two
eNodeBs, the function will create an X2 interface between every pair of eNodeBs
in the container.

Lastly, the target eNodeB must be configured as "open" to X2 HANDOVER REQUEST.
Every eNodeB is open by default, so no extra instruction is needed in most
cases. However, users may set the eNodeB to "closed" by setting the boolean
attribute ``LteEnbRrc::AdmitHandoverRequest`` to `false`. As an example, you can
run the ``lena-x2-handover`` program and setting the attribute in this way::

   NS_LOG=EpcX2:LteEnbRrc ./waf --run lena-x2-handover --command="%s --ns3::LteEnbRrc::AdmitHandoverRequest=false"

After the above three requirements are fulfilled, the handover procedure can be
triggered manually or automatically. Each will be presented in the following
subsections.


Manual handover trigger
***********************

Handover event can be triggered "manually" within the simulation program by
scheduling an explicit handover event. The ``LteHelper`` object provides a
convenient method for the scheduling of a handover event. As an example, let us
assume that ``ueLteDevs`` is a ``NetDeviceContainer`` that contains the UE that
is to be handed over, and that ``enbLteDevs`` is another ``NetDeviceContainer``
that contains the source and the target eNB. Then, a handover at 0.1s can be
scheduled like this::

   lteHelper->HandoverRequest (Seconds (0.100), 
                               ueLteDevs.Get (0), 
                               enbLteDevs.Get (0), 
                               enbLteDevs.Get (1));

Note that the UE needs to be already connected to the source eNB, otherwise the
simulation will terminate with an error message. 

For an example with full source code, please refer to the ``lena-x2-handover``
example program.


.. _sec-automatic-handover:

Automatic handover trigger
**************************

Handover procedure can also be triggered "automatically" by the serving eNodeB 
of the UE. The logic behind the trigger depends on the handover algorithm
currently active in the eNodeB RRC entity. Users may select and configure the
handover algorithm that will be used in the simulation, which will be explained
shortly in this section. Users may also opt to write their own implementation of
handover algorithm, as described in Section :ref:`sec-handover-algorithm` of the
Design Documentation.

Selecting a handover algorithm is done via the ``LteHelper`` object and its
``SetHandoverAlgorithmType`` method as shown below::

   Ptr<LteHelper> lteHelper = CreateObject<LteHelper> ();
   lteHelper->SetHandoverAlgorithmType ("ns3::A2A4RsrqHandoverAlgorithm");
 
The selected handover algorithm may also provide several configurable
attributes, which can be set as follows::

   lteHelper->SetHandoverAlgorithmAttribute ("ServingCellThreshold",
                                             UintegerValue (30));
   lteHelper->SetHandoverAlgorithmAttribute ("NeighbourCellOffset",
                                             UintegerValue (1));

Three options of handover algorithm are included in the LTE module. The
*A2-A4-RSRQ* handover algorithm (named as ``ns3::A2A4RsrqHandoverAlgorithm``) is
the default option, and the usage has already been shown above.

Another option is the *strongest cell* handover algorithm (named as
``ns3::A3RsrpHandoverAlgorithm``), which can be selected and configured by the
following code::

   lteHelper->SetHandoverAlgorithmType ("ns3::A3RsrpHandoverAlgorithm");
   lteHelper->SetHandoverAlgorithmAttribute ("Hysteresis",
                                             DoubleValue (3.0));
   lteHelper->SetHandoverAlgorithmAttribute ("TimeToTrigger",
                                             TimeValue (MilliSeconds (256)));

The last option is a special one, called the *no-op* handover algorithm, which
basically disables automatic handover trigger. This is useful for example in
cases where manual handover trigger need an exclusive control of all handover
decision. It does not have any configurable attributes. The usage is as
follows::

   lteHelper->SetHandoverAlgorithmType ("ns3::NoOpHandoverAlgorithm");

For more information on each handover algorithm's decision policy and their
attributes, please refer to their respective subsections in Section
:ref:`sec-handover-algorithm` of the Design Documentation.

Finally, the ``InstallEnbDevice`` function of ``LteHelper`` will instantiate one
instance of the selected handover algorithm for each eNodeB device. In other
words, make sure to select the right handover algorithm before finalizing it in
the following line of code::

   NetDeviceContainer enbLteDevs = lteHelper->InstallEnbDevice (enbNodes); 

Example with full source code of using automatic handover trigger can be found
in the ``lena-x2-handover-measures`` example program.


.. _sec-tuning-handover-simulation:

Tuning simulation with handover
*******************************

As mentioned in the Design Documentation, the current implementation of handover
model may produce unpredicted behaviour when handover failure occurs. This
subsection will focus on the steps that should be taken into account by users
if they plan to use handover in their simulations.

The major cause of handover failure that we will tackle is the error in
transmitting handover-related signaling messages during the execution of a
handover procedure. As apparent from the Figure
:ref:`fig-x2-based-handover-seq-diagram` from the Design Documentation, there
are many of them and they use different interfaces and protocols. For the sake
of simplicity, we can safely assume that the X2 interface (between the source
eNodeB and the target eNodeB) and the S1 interface (between the target eNodeB
and the SGW/PGW) are quite stable. Therefore we will focus our attention to the
RRC protocol (between the UE and the eNodeBs) and the Random Access procedure,
which are normally transmitted through the air and susceptible to degradation of
channel condition. 

A general tips to reduce transmission error is to *ensure high enough SINR*
level in every UE. This can be done by a proper planning of the network topology
that *minimizes network coverage hole*. If the topology has a known coverage
hole, then the UE should be configured not to venture to that area.

Another approach to keep in mind is to *avoid too-late handovers*. In other
words, handover should happen before the UE's SINR becomes too low, otherwise
the UE may fail to receive the handover command from the source eNodeB. Handover
algorithms have the means to control how early or late a handover decision is
made. For example, A2-A4-RSRQ handover algorithm can be configured with a higher
threshold to make it decide a handover earlier. Similarly, smaller hysteresis
and/or shorter time-to-trigger in the strongest cell handover algorithm
typically results in earlier handovers. In order to find the right values for
these parameters, one of the factors that should be considered is the UE
movement speed. Generally, a faster moving UE requires the handover to be
executed earlier. Some research work have suggested recommended values, such as
in [Lee2010]_.

The above tips should be enough in normal simulation uses, but in the case some
special needs arise then an extreme measure can be taken into consideration.
For instance, users may consider *disabling the channel error models*. This will
ensure that all handover-related signaling messages will be transmitted
successfully, regardless of distance and channel condition. However, it will
also affect all other data or control packets not related to handover, which may
be an unwanted side effect. Otherwise, it can be done as follows::

   Config::SetDefault ("ns3::LteSpectrumPhy::CtrlErrorModelEnabled");
   Config::SetDefault ("ns3::LteSpectrumPhy::DataErrorModelEnabled");
   
By using the above code, we disable the error model in both control and data
channels and in both directions (downlink and uplink). This is necessary because
handover-related signaling messages are transmitted using these channels. An
exception is when the simulation uses the ideal RRC protocol. In this case, only
the Random Access procedure is left to be considered. The procedure consists of
control messages, therefore we only need to disable the control channel's error
model.
      

.. _sec-handover-traces:

Handover traces
***************

The RRC model, in particular the ``LteEnbRrc`` and ``LteUeRrc``
objects, provide some useful traces which can be hooked up to some
custom functions so that they are called upon start and end of the
handover execution phase at both the UE and eNB side. As an example,
in your simulation program you can declare the following methods::

   void 
   NotifyHandoverStartUe (std::string context, 
                          uint64_t imsi, 
                          uint16_t cellId, 
                          uint16_t rnti, 
                          uint16_t targetCellId)
   {
     std::cout << Simulator::Now ().GetSeconds () << " " << context 
               << " UE IMSI " << imsi 
               << ": previously connected to CellId " << cellId 
               << " with RNTI " << rnti 
               << ", doing handover to CellId " << targetCellId 
               << std::endl;
   }

   void 
   NotifyHandoverEndOkUe (std::string context, 
                          uint64_t imsi, 
                          uint16_t cellId, 
                          uint16_t rnti)
   {
     std::cout << Simulator::Now ().GetSeconds () << " " << context 
               << " UE IMSI " << imsi 
               << ": successful handover to CellId " << cellId 
               << " with RNTI " << rnti 
               << std::endl;
   }

   void 
   NotifyHandoverStartEnb (std::string context, 
                           uint64_t imsi, 
                           uint16_t cellId, 
                           uint16_t rnti, 
                           uint16_t targetCellId)
   {
     std::cout << Simulator::Now ().GetSeconds () << " " << context 
               << " eNB CellId " << cellId 
               << ": start handover of UE with IMSI " << imsi 
               << " RNTI " << rnti 
               << " to CellId " << targetCellId 
               << std::endl;
   }

   void 
   NotifyHandoverEndOkEnb (std::string context, 
                           uint64_t imsi, 
                           uint16_t cellId, 
                           uint16_t rnti)
   {
     std::cout << Simulator::Now ().GetSeconds () << " " << context 
               << " eNB CellId " << cellId 
               << ": completed handover of UE with IMSI " << imsi 
               << " RNTI " << rnti 
               << std::endl;
   }

Then, you can hook up these methods to the corresponding trace sources
like this::

   Config::Connect ("/NodeList/*/DeviceList/*/LteEnbRrc/HandoverStart",
                    MakeCallback (&NotifyHandoverStartEnb));
   Config::Connect ("/NodeList/*/DeviceList/*/LteUeRrc/HandoverStart",
                    MakeCallback (&NotifyHandoverStartUe));
   Config::Connect ("/NodeList/*/DeviceList/*/LteEnbRrc/HandoverEndOk",
                    MakeCallback (&NotifyHandoverEndOkEnb));
   Config::Connect ("/NodeList/*/DeviceList/*/LteUeRrc/HandoverEndOk",
                    MakeCallback (&NotifyHandoverEndOkUe));

The example program ``src/lte/examples/lena-x2-handover.cc``
illustrates how the all above instructions can be integrated in a
simulation program. You can run the program like this::

   ./waf --run lena-x2-handover

and it will output the messages printed by the custom handover trace
hooks. In order additionally visualize some meaningful logging
information, you can run the program like this::

    NS_LOG=LteEnbRrc:LteUeRrc:EpcX2 ./waf --run lena-x2-handover





Examples Programs
-----------------

The directory ``src/lte/examples/`` contains some example simulation programs that
show how to simulate different LTE scenarios. 



Reference scenarios
-------------------

There is a vast amount of reference LTE simulation scenarios which can
be found in the literature. Here we list some of them: 

 * The system simulation scenarios mentioned in section A.2 of [TR36814]_.

 * The dual stripe model [R4-092042]_, which is partially implemented in the
   example program ``src/lte/examples/lena-dual-stripe.cc``. This example
   program features a lot of configurable parameters which can be customized by
   changing the corresponding global variables. To get a list of all these
   global variables, you can run this command::

     ./waf --run lena-dual-stripe --command-template="%s --PrintGlobals"
     
   The following subsection presents an example of running a simulation
   campaign using this example program.


Handover simulation campaign
****************************

In this subsection, we will demonstrate an example of running a simulation
campaign using the LTE module of |ns3|. The objective of the campaign is to
compare the effect of each built-in handover algorithm of the LTE module.

The campaign will use the ``lena-dual-stripe`` example program. First, we have
to modify the example program to produce the output that we need. In this
occassion, we want to produce the number of handovers, user average throughput,
and average SINR.

The number of handovers can be obtained by counting the number of times the
`HandoverEndOk` :ref:`sec-handover-traces` is fired. Then the user average
throughput can be obtained by enabling the RLC :ref:`sec-simulation-output`.
Finally, SINR can be obtained by enabling the PHY simulation output. The
following sample code snippet shows one possible way to obtain the above::

   void
   NotifyHandoverEndOkUe (std::string context, uint64_t imsi,
                          uint16_t cellId, uint16_t rnti)
   {
     std::cout << "Handover IMSI " << imsi << std::endl;
   }

   int
   main (int argc, char *argv[])
   {
     /*** SNIP ***/

     Config::Connect ("/NodeList/*/DeviceList/*/LteUeRrc/HandoverEndOk",
                      MakeCallback (&NotifyHandoverEndOkUe));

     lteHelper->EnablePhyTraces ();
     lteHelper->EnableRlcTraces ();
     Ptr<RadioBearerStatsCalculator> rlcStats = lteHelper->GetRlcStats ();
     rlcStats->SetAttribute ("StartTime", TimeValue (Seconds (0)));
     rlcStats->SetAttribute ("EpochDuration", TimeValue (Seconds (simTime)));

     Simulator::Run ();
     Simulator::Destroy ();
     return 0;
   }

Then we have to configure the parameters of the program to suit our simulation
needs. We are looking for the following assumptions in our simulation:

 * 7 sites of tri-sectored macro eNodeBs (i.e. 21 macrocells) deployed in
   hexagonal layout with 500 m inter-site distance.

 * Although ``lena-dual-stripe`` is originally intended for a two-tier
   (macrocell and femtocell) simulation, we will simplify our simulation to
   one-tier (macrocell) simulation only.

 * UEs are randomly distributed around the sites and attach to the network
   automatically using Idle mode cell selection. After that, UE will roam the
   simulation environment with 60 kmph movement speed.

 * 50 seconds simulation duration, so UEs would have traveled far enough to
   trigger some handovers.

 * 46 dBm macrocell Tx power and 10 dBm UE Tx power.

 * EPC mode will be used because the X2 handover procedure requires it to be
   enabled.

 * Full-buffer downlink and uplink traffic, both in 5 MHz bandwidth, using TCP
   protocol and Proportional Fair scheduler.

 * Ideal RRC protocol.

Table :ref:`tab-handover-campaign-program-parameter` below shows how we
configure the parameters of ``lena-dual-stripe`` to achieve the above
assumptions.

.. _tab-handover-campaign-program-parameter:

.. table:: ``lena-dual-stripe`` parameter configuration for handover campaign

   ================== ========== ===============================================
   Parameter name     Value      Description
   ================== ========== ===============================================
   simTime            50         50 seconds simulation duration
   nBlocks            0          Disabling apartment buildings and femtocells
   nMacroEnbSites     7          Number of macrocell sites (each site has 3
                                 cells)
   nMacroEnbSitesX    2          The macrocell sites will be positioned in a
                                 2-3-2 formation
   interSiteDistance  500        500 m distance between adjacent macrocell sites
   macroEnbTxPowerDbm 46         46 dBm Tx power for each macrocell
   epc                1          Enable EPC mode
   epcDl              1          Enable full-buffer DL traffic
   epcUl              1          Enable full-buffer UL traffic
   useUdp             0          Disable UDP traffic and enable TCP instead
   macroUeDensity     0.00002    Determines number of UEs (translates to 48 UEs
                                 in our simulation)
   outdoorUeMinSpeed  16.6667    Minimum UE movement speed in m/s (60 kmph)
   outdoorUeMaxSpeed  16.6667    Maximum UE movement speed in m/s (60 kmph)
   macroEnbBandwidth  25         5 MHz DL and UL bandwidth
   generateRem        1          (Optional) For plotting the Radio Environment
                                 Map
   ================== ========== ===============================================

Some of the required assumptions are not available as parameters of
``lena-dual-stripe``. In this case, we override the default attributes, as
shown in Table :ref:`tab-handover-campaign-default-values` below.

.. _tab-handover-campaign-default-values:

.. table:: Overriding default attributes for handover campaign

   ==================================================== ================================== ==============================================
   Default value name                                   Value                              Description
   ==================================================== ================================== ==============================================
   ns3::LteHelper::HandoverAlgorithm                    `ns3::NoOpHandoverAlgorithm`,      Choice of handover algorithm
                                                        `ns3::A3RsrpHandoverAlgorithm`, or
                                                        `ns3::A2A4RsrqHandoverAlgorithm`
   ns3::LteHelper::Scheduler                            `ns3::PfFfMacScheduler`            Proportional Fair scheduler
   ns3::LteHelper::UseIdealRrc                           1                                 Ideal RRC protocol
   ns3::RadioBearerStatsCalculator::DlRlcOutputFilename `<run>`-DlRlcStats.txt             File name for DL RLC trace output
   ns3::RadioBearerStatsCalculator::UlRlcOutputFilename `<run>`-UlRlcStats.txt             File name for UL RLC trace output
   ns3::PhyStatsCalculator::DlRsrpSinrFilename          `<run>`-DlRsrpSinrStats.txt        File name for DL PHY RSRP/SINR trace output
   ns3::PhyStatsCalculator::UlSinrFilename              `<run>`-UlSinrStats.txt            File name for UL PHY SINR trace output
   ==================================================== ================================== ==============================================

|ns3| provides many ways for passing configuration values into a simulation. In
this example, we will use the command line arguments. It is basically done by
appending the parameters and their values to the ``waf`` call when starting each
individual simulation. So the ``waf`` calls for invoking our 3 simulations would
look as below::

   $ ./waf --run="lena-dual-stripe
     --simTime=50 --nBlocks=0 --nMacroEnbSites=7 --nMacroEnbSitesX=2
     --epc=1 --useUdp=0 --outdoorUeMinSpeed=16.6667 --outdoorUeMaxSpeed=16.6667
     --ns3::LteHelper::HandoverAlgorithm=ns3::NoOpHandoverAlgorithm
     --ns3::RadioBearerStatsCalculator::DlRlcOutputFilename=no-op-DlRlcStats.txt
     --ns3::RadioBearerStatsCalculator::UlRlcOutputFilename=no-op-UlRlcStats.txt
     --ns3::PhyStatsCalculator::DlRsrpSinrFilename=no-op-DlRsrpSinrStats.txt
     --ns3::PhyStatsCalculator::UlSinrFilename=no-op-UlSinrStats.txt
     --RngRun=1" > no-op.txt

   $ ./waf --run="lena-dual-stripe
     --simTime=50 --nBlocks=0 --nMacroEnbSites=7 --nMacroEnbSitesX=2
     --epc=1 --useUdp=0 --outdoorUeMinSpeed=16.6667 --outdoorUeMaxSpeed=16.6667
     --ns3::LteHelper::HandoverAlgorithm=ns3::A3RsrpHandoverAlgorithm
     --ns3::RadioBearerStatsCalculator::DlRlcOutputFilename=a3-rsrp-DlRlcStats.txt
     --ns3::RadioBearerStatsCalculator::UlRlcOutputFilename=a3-rsrp-UlRlcStats.txt
     --ns3::PhyStatsCalculator::DlRsrpSinrFilename=a3-rsrp-DlRsrpSinrStats.txt
     --ns3::PhyStatsCalculator::UlSinrFilename=a3-rsrp-UlSinrStats.txt
     --RngRun=1" > a3-rsrp.txt

   $ ./waf --run="lena-dual-stripe
     --simTime=50 --nBlocks=0 --nMacroEnbSites=7 --nMacroEnbSitesX=2
     --epc=1 --useUdp=0 --outdoorUeMinSpeed=16.6667 --outdoorUeMaxSpeed=16.6667
     --ns3::LteHelper::HandoverAlgorithm=ns3::A2A4RsrqHandoverAlgorithm
     --ns3::RadioBearerStatsCalculator::DlRlcOutputFilename=a2-a4-rsrq-DlRlcStats.txt
     --ns3::RadioBearerStatsCalculator::UlRlcOutputFilename=a2-a4-rsrq-UlRlcStats.txt
     --ns3::PhyStatsCalculator::DlRsrpSinrFilename=a2-a4-rsrq-DlRsrpSinrStats.txt
     --ns3::PhyStatsCalculator::UlSinrFilename=a2-a4-rsrq-UlSinrStats.txt
     --RngRun=1" > a2-a4-rsrq.txt

Some notes on the execution:

 * Notice that some arguments are not specified because they are already the
   same as the default values. We also keep the handover algorithms on each own
   default settings.

 * Note the file names of simulation output, e.g. RLC traces and PHY traces,
   because we have to make sure that they are not overwritten by the next
   simulation run. In this example, we specify the names one by one using the
   command line arguments.

 * The ``--RngRun=1`` argument at the end is used for setting the run number
   used by the random number generator used in the simulation. We re-run the
   same simulations with different `RngRun` values, hence creating several
   independent replications of the same simulations. Then we average the
   results obtained from these replications to achieve some statistical
   confidence.

 * We can add a ``--generateRem=1`` argument to generate the files necessary for
   generating the Radio Environment Map (REM) of the simulation. The result is
   Figure :ref:`fig-lte-handover-campaign-rem` below, which can be produced by
   following the steps described in Section :ref:`sec-radio-environment-maps`.
   This figure also shows the position of eNodeBs and UEs at the beginning of a
   simulation using ``RngRun = 1``. Other values of `RngRun` may produce
   different UE position.
   
.. _fig-lte-handover-campaign-rem:

.. figure:: figures/lte-handover-campaign-rem.*
   :align: center

   REM obtained from a simulation in handover campaign

After hours of running, the simulation campaign will eventually end. Next we
will perform some post-processing on the produced simulation output to obtain
meaningful information out of it.

In this example, we use GNU Octave to assist the processing of throughput and
SINR data, as demonstrated in a sample GNU Octave script below::

   % RxBytes is the 10th column
   DlRxBytes = load ("no-op-DlRlcStats.txt") (:,10);
   DlAverageThroughputKbps = sum (DlRxBytes) * 8 / 1000 / 50

   % RxBytes is the 10th column
   UlRxBytes = load ("no-op-UlRlcStats.txt") (:,10);
   UlAverageThroughputKbps = sum (UlRxBytes) * 8 / 1000 / 50

   % Sinr is the 6th column
   DlSinr = load ("no-op-DlRsrpSinrStats.txt") (:,6);
   % eliminate NaN values
   idx = isnan (DlSinr);
   DlSinr (idx) = 0;
   DlAverageSinrDb = 10 * log10 (mean (DlSinr)) % convert to dB

   % Sinr is the 5th column
   UlSinr = load ("no-op-UlSinrStats.txt") (:,5);
   % eliminate NaN values
   idx = isnan (UlSinr);
   UlSinr (idx) = 0;
   UlAverageSinrDb = 10 * log10 (mean (UlSinr)) % convert to dB

As for the number of handovers, we can use simple shell scripting to count the
number of occurrences of string "Handover" in the log file::

   $ grep "Handover" no-op.txt | wc -l

Table :ref:`tab-handover-campaign-results` below shows the complete statistics
after we are done with post-processing on every individual simulation run. The
values shown are the average of the results obtained from ``RngRun`` of 1, 2, 3,
and 4.

.. _tab-handover-campaign-results:

.. table:: Results of handover campaign

   ===================================== ========== =========== ==============
   Statistics                            No-op      A2-A4-RSRQ  Strongest cell
   ===================================== ========== =========== ==============
   Average DL system throughput          6 615 kbps 20 509 kbps 19 709 kbps
   Average UL system throughput          4 095 kbps 5 705 kbps  6 627 kbps
   Average DL SINR                       -0.10 dB   5.19 dB     5.24 dB
   Average UL SINR                       9.54 dB    81.57 dB    79.65 dB
   Number of handovers per UE per second 0          0.05694     0.04771
   ===================================== ========== =========== ==============

.. Below are the detailed datasheets from the campaign, for informational
   purpose, but hidden from the published document.

.. ======================= ========== ========== ========== ========== =======
   NoOp                    RngRun = 1 RngRun = 2 RngRun = 3 RngRun = 4 Average
   ======================= ========== ========== ========== ========== =======
   DlAverageThroughputKbps 8 476      4 478      6 913      6 593      6 615
   UlAverageThroughputKbps 4 923      2 962      4 715      3 779      4 095
   DlAverageSinrDb         0.40       -0.99      0.84       -0.64      -0.10
   UlAverageSinrDb         7.93       8.06       12.52      9.65       9.54
   NumHandoverPerUePerSec  0          0          0          0          0
   ======================= ========== ========== ========== ========== =======

.. ======================= ========== ========== ========== ========== =======
   A2A4Rsrq                RngRun = 1 RngRun = 2 RngRun = 3 RngRun = 4 Average
   ======================= ========== ========== ========== ========== =======
   DlAverageThroughputKbps 21 575     18 500     n/a        21 451     20 509
   UlAverageThroughputKbps 6 039      5 320      n/a        5 757      5 705
   DlAverageSinrDb         5.31       5.16       n/a        5.09       5.19
   UlAverageSinrDb         84.17      79.18      n/a        81.37      81.57
   NumHandoverPerUePerSec  0.05458    0.06000    n/a        0.05625    0.05694
   ======================= ========== ========== ========== ========== =======
   RngRun = 3 simulation got a segmentation fault as around +15.2s. The cause is
   unknown at the moment.

.. ======================= ========== ========== ========== ========== =======
   A3Rsrp                  RngRun = 1 RngRun = 2 RngRun = 3 RngRun = 4 Average
   ======================= ========== ========== ========== ========== =======
   DlAverageThroughputKbps 20 349     17 781     20 229     20 478     19 709
   UlAverageThroughputKbps 6 491      6 397      7 555      6 064      6 627
   DlAverageSinrDb         5.24       5.08       5.63       5.01       5.24
   UlAverageSinrDb         83.62      81.94      78.84      74.19      79.65
   NumHandoverPerUePerSec  0.04625    0.04917    0.04958    0.04583    0.04771
   ======================= ========== ========== ========== ========== =======

The results show that having a handover algorithm in a mobility simulation
improves both user throughput and SINR significantly. There is little difference
between the two handover algorithms in this campaign scenario. It would be
interesting to see their performance in different scenarios, such as scenarios
with home eNodeBs deployment.
