|  |
| --- |
| **Table S5 The comparison of the results of the proposed method by putting aside different components on the Car-front sequence based on the SSIM and PSNR criteria.** |
| Criteria | The proposed method without distortion detection | The proposed method without blur removal | The proposed method without RANSAC procedure | The proposed method |
| SSIM | 0.6919 | 0.7612 | 0.8207 | 0.9460 |
| PSNR | 17.74 | 18.66 | 20.67 | 25.1344 |