Chronologic VCS simulator copyright 1991-2020
Contains Synopsys proprietary information.
Compiler version R-2020.12-1_Full64; Runtime version R-2020.12-1_Full64;  Oct 13 10:53 2023
[UART] UART0 is here (stdin/stdout).
mcycle = 1005195
minstret = 559203
$finish called from file "/proj/users/hanwei.fan/dataset/generated-src/chipyard.harness.TestHarness.Boom64n8n128n16n2n4n128n2n2n1n4/gen-collateral/TestDriver.v", line 158.
$finish at simulation time           5185385500
           V C S   S i m u l a t i o n   R e p o r t 
Time: 5185385500 ps
CPU Time:   1450.910 seconds;       Data structure size:   3.2Mb
Fri Oct 13 11:17:46 2023
