Chronologic VCS simulator copyright 1991-2020
Contains Synopsys proprietary information.
Compiler version R-2020.12-1_Full64; Runtime version R-2020.12-1_Full64;  Nov 14 03:15 2023
[UART] UART0 is here (stdin/stdout).
mcycle = 139162
minstret = 119202
$finish called from file "/proj/users/hanwei.fan/dataset/generated-src/chipyard.harness.TestHarness.Boom16n2n2048n8n10n5n64n1n5n2n16/gen-collateral/TestDriver.v", line 158.
$finish at simulation time           2411885500
           V C S   S i m u l a t i o n   R e p o r t 
Time: 2411885500 ps
CPU Time:    283.030 seconds;       Data structure size:   6.2Mb
Tue Nov 14 03:20:22 2023
