Chronologic VCS simulator copyright 1991-2020
Contains Synopsys proprietary information.
Compiler version R-2020.12-1_Full64; Runtime version R-2020.12-1_Full64;  Nov 16 23:25 2023
[UART] UART0 is here (stdin/stdout).
Shortest path is 80 in cost. 
mcycle = 1393844
minstret = 1307572
$finish called from file "/proj/users/hanwei.fan/dataset/generated-src/chipyard.harness.TestHarness.Boom32n2n128n2n2n1n32n1n1n1n4/gen-collateral/TestDriver.v", line 158.
$finish at simulation time           8241215500
           V C S   S i m u l a t i o n   R e p o r t 
Time: 8241215500 ps
CPU Time:    951.260 seconds;       Data structure size:   2.2Mb
Thu Nov 16 23:41:43 2023
