Chronologic VCS simulator copyright 1991-2020
Contains Synopsys proprietary information.
Compiler version R-2020.12-1_Full64; Runtime version R-2020.12-1_Full64;  Nov 18 16:10 2023
[UART] UART0 is here (stdin/stdout).
mcycle = 1420054
minstret = 1069712
$finish called from file "/proj/users/hanwei.fan/dataset/generated-src/chipyard.harness.TestHarness.Boom16n4n128n2n6n4n160n2n2n1n8/gen-collateral/TestDriver.v", line 158.
$finish at simulation time           3435745500
           V C S   S i m u l a t i o n   R e p o r t 
Time: 3435745500 ps
CPU Time:   1057.630 seconds;       Data structure size:   3.1Mb
Sat Nov 18 16:28:03 2023
