Chronologic VCS simulator copyright 1991-2020
Contains Synopsys proprietary information.
Compiler version R-2020.12-1_Full64; Runtime version R-2020.12-1_Full64;  Nov 16 21:21 2023
[UART] UART0 is here (stdin/stdout).
mcycle = 1541911
minstret = 1327133
$finish called from file "/proj/users/hanwei.fan/dataset/generated-src/chipyard.harness.TestHarness.Boom16n2n256n16n6n3n32n1n3n1n4/gen-collateral/TestDriver.v", line 158.
$finish at simulation time           4347035500
           V C S   S i m u l a t i o n   R e p o r t 
Time: 4347035500 ps
CPU Time:   1170.410 seconds;       Data structure size:   3.2Mb
Thu Nov 16 21:40:48 2023
