**%Error**

= ((sum of measurements / n)-true value) / true value)\*100%

= ((91.61-91.44)/91.44) \*100%1

=0.2%

1. 91.44 = length in meters of American football field